Input signal *v*:

A number of measurements:

Pseudoinverse solution for an overdetermined system: